SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( BKD_Tw6a_Eaos_pr_1
 Type ( Freight )
 WagonShape ( Tw6a.s )
 FreightAnim (y25-stat.s 1 1 )
  Name ("BKD_Tw6a-Eaos pusty[1b]")
 Size ( 1.85m 0.57m 7.35m )
 Mass ( 18.6t )
 WheelRadius ( 0.225m )
 InertiaTensor ( Box (1.85m 0.57m 7.35m) )
Coupling (
Type ( Bar )
  Spring (
   Stiffness ( 7.5e6N/m 1e7N/m )
   Damping ( 1e6N/m/s 2e6N/m/s )
   Break ( 1.1e8N 5e8N )
   r0 ( 80cm 150cm )
          )
  CouplingHasRigidConnection ( 1 )
  Velocity ( 0.01m/s )
 )
 Coupling (
  Type ( Chain )
  CouplerUniqueType ( Tw6a )
  Spring (
   Stiffness ( 7.5e6N/m 1e7N/m )
   Damping ( 1e6N/m/s 2e6N/m/s )
   Break ( 1.1e8N 5e8N )
   r0 ( 80cm 150cm )
          )
  CouplingHasRigidConnection ( 1 )
  Velocity ( 0.01m/s )
 )

 Buffers (
  Spring (
   Stiffness ( 1e6N/m 5e6N/m )
   Damping ( 1e6N/m/s 1e6N/m/s )
   r0 ( 0m 1e9 )
  )
  Centre ( 0.5 )
  Radius ( 1 )
  Angle ( 0.5deg )
 )

 Adheasion ( 0.2533   0.8233   2.5263   0 )
  comment ( Adhesion computed with NW(8) by TS-FastFix)
 DerailRailHeight ( 4cm )
 DerailRailForce ( 18.6kN )
 DerailBufferForce ( 400kN )
 NumWheels(6)
Friction (
 620.6N/m/s    -0.10    1.5mph    1.188N/m/s    1.999
  5.1N/rad/s  1  -1rad/s  0  1
 )
comment( Friction modified with FCalc 2.0 by Joseph T. Realmuto.
 
   Rail Unit Type : Roller Bearing Freight Car
   Speed Range    : 13 mph / 20 kph
   Number of Axles: 6
   Weight         : 18.6t (8t tara Tw6a + 10,6t tara 430Wa + 0t netto)
   Frontal Area   : 5.42 m2)

 BrakeEquipmentType ( "Handbrake, Distributor, Auxilary_reservoir, Emergency_brake_reservoir" )
 BrakeSystemType ( "Air_single_pipe" )
 MaxBrakeForce( 18kN )

 MaxHandbrakeForce( 15kN )
 NumberOfHandbrakeLeverSteps( 100 )

 BrakeDistributorFullServicePressure( 50.76 )
 BrakeDistributorEmergencyApplicationPressure( 50.76 )
 BrakeDistributorMaxAuxilaryResPressure( 72.6 )
 BrakeDistributorEmergencyResPressure( 72.6 )
 BrakeDistributorReleaseRate( 2.5 )
 BrakeDistributorApplicationRate( 2.5 )
 BrakeDistributorTrainPipeControlRatio( 2.33 )
 BrakeDistributorNormalFullReleasePressure( 72.6 )

 TripleValveRatio( 2.33 )
 MaxReleaseRate( 2.5 )
 MaxApplicationRate( 2.5 )
 MaxAuxilaryChargingRate( 5 )
 EmergencyResCapacity( 7 )
 EmergencyResChargingRate( 5 )
 EmergencyBrakeResMaxPressure( 50.76 )
 BrakeCylinderPressureForMaxBrakeBrakeForce( 50.76 )

   Sound ( "..//..//BKD_SOUND//Schmalspurwag-6x.sms" )

)