SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( Lxd2-255trfB
 Type ( Engine)
 comment( the model of the diesel-hydraulic narrow gauge 750 mm locomotive L45H after a major repair
          with a refurbished engine Henschel Wola 71H12A 371 kW with its original factory specifications)
 WagonShape ( BKD_Lxd2-255trfB.s )
 Size ( 2.35m 3.25m 9.82m)
 Mass ( 32t)
 WheelRadius ( 0.375m)
 InertiaTensor (
  Box ( 3.2m 4.12m 10.34m)
 )

Coupling (
  Type ( Chain )
  Spring (
   Stiffness ( 7.5e6N/m 1e7N/m )
   Damping ( 1e6N/m/s 2e6N/m/s )
   Break ( 1.1e8N 5e8N )
   r0 ( 80cm 150cm )
          )
  CouplingHasRigidConnection (1)
  Velocity ( 0.01m/s )
 )
 Buffers (
  Spring (
   Stiffness ( 1e6N/m 5e6N/m )
   Damping ( 1e6N/m/s 1e6N/m/s )
   r0 ( 80cm 150cm )
  )
  Centre ( 0.5m )
  Radius ( 1m )
  Angle ( 0.5deg )
 )

 Adheasion ( 0.1 0.62 2 0)
 DerailRailHeight ( 10cm)
 DerailRailForce ( 80kN) comment( 2.5*32t)
 DerailBufferForce ( 400kN)
 NumWheels ( 4 )
 
 Friction ( 721N/m/s 0 1mph 9.42N/m/s 1.8 5.1N/rad/s 1 -1rad/s 0 1)
 comment( calculated on the friction calculator program Fcalc 10 )
 
 AntiSlip ( 1)
 
 BrakeEquipmentType ( "Triple_valve, Auxilary_reservoir, Emergency_brake_reservoir" )
 BrakeSystemType ( Air_single_pipe)
 MaxBrakeForce ( 31kN) comment(brake adjustment "P" = (brake mass 32t x 9,82) x 0,1)
 TripleValveRatio ( 2.33)
 MaxReleaseRate ( 4)
 MaxApplicationRate ( 2)
 EmergencyResCapacity( 10 )
 EmergencyResChargingRate( 15 )
 MaxAuxilaryChargingRate ( 20)
 EmergencyBrakeResMaxPressure( 50.76 )
 BrakeCylinderPressureForMaxBrakeBrakeForce ( 50.76) comment(8 inch brake cylinder)

 IntakePoint ( -4.5 2 FuelDiesel)
 IntakePoint ( 4.5 2 FuelDiesel)
 Lights ( 4
Light (
   comment ( AI Biale gorne przednie )
   Type ( 0)
   Conditions (
   Control ( 1 )
   Unit ( 2 )
   Service ( 2 )
   )

   FadeIn ( 0.5)
   FadeOut ( 0.5)
   Cycle ( 0)
   States ( 1
    State (
     Duration ( 0)
     LightColour ( 80FFFFFF)
     Position ( 0 2.96 4.81)
     Azimuth ( 0 0 0 )
     Transition ( 0)
     Radius ( 0.35)
    )
   )
  )
  Light (
   comment ( AI Biale prawe przednie )
   Type ( 0)
   Conditions ( 
   Control ( 1 )
   Unit ( 2 )
   Service ( 2 )
   )

   FadeIn ( 0.5)
   FadeOut ( 0.5)
   Cycle ( 0)
   States ( 1
    State (
     Duration ( 0)
     LightColour ( fff3e1a1)
     Position ( 0.57 1.36 4.7)
     Azimuth ( 0 0 0 )
     Transition ( 0)
     Radius ( 0.2)
    )
   )
  )
  Light (
   comment ( AI Biale lewe przednie )
   Type ( 0)
  Conditions ( 
  Control ( 1 )
  Unit ( 2 )
  Service ( 2 )
  )

   FadeIn ( 0.5)
   FadeOut ( 0.5)
   Cycle ( 0)
   States ( 1
    State (
     Duration ( 0)
     LightColour ( fff3e1a1)
     Position ( -0.57 1.36 4.7)
     Azimuth ( 0 0 0 )
     Transition ( 0)
     Radius ( 0.2)
    )
   )
  )
Light (
   comment ( AI Czerwone prawe tylne )
   Type ( 0)
   Conditions (
	Control ( 1 )
    Headlight ( 3 )
    Unit ( 2 )
   )
   FadeIn ( 0.5)
   FadeOut ( 0.5)
   Cycle ( 0)
   States ( 1
    State (
     Duration ( 0)
     LightColour ( FFFF0000)
     Position ( 0.57 1.36 -4.7)
     Azimuth ( -180 -180 -180)
     Transition ( 0)
     Radius ( 0.2)
    )
   )
  )
)


Sound ( "Lxd2eng_wola.sms" )
)

Engine (Lxd2-255trfB
 Effects (
  DieselSpecialEffects (
     Exhaust1
   (
                    0.1 3.4 -0.7
    0 1 0
    0.02   )
    )
 )
 Wagon (Lxd2-255trfB)
 Type ( Diesel)
 MaxPower ( 280kW )
 MaxForce ( 150kN)
 MaxContinuousForce ( 150kN)
 MaxVelocity ( 18.5mph)
 MaxCurrent ( 1000A)
 WheelRadius ( 20in)
 Sanding ( 1E9mph)
 NumWheels ( 4)
 MaxTemperature ( 90°C)
 MaxOilPressure ( 64psi)
 HeadOut ( 1.3m 2.65m -2.075m)
 	AirBrakesAirCompressorPowerRating( 0.58 )
	AirBrakesMainMinResAirPressure( 0 )
	AirBrakesMainMaxAirPressure( 108.5 )
	AirBrakesMainResVolume( 6.71 )
	AirBrakesAirCompressorWattage( 17000W )
	AirBrakesCompressorRestartPressure( 92.45 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 2 )
		AirBrakesHasLowPressureTest( 0 )
	AirBrakesIsCompressorElectricOrMechanical( 1 )
        AirBrakesMaxMainResPipePressure ( 72.6 )

	EngineBrakesControllerMinPressureReduction( 6 )
	EngineBrakesControllerHasProportionalBrake( 1 )
	EngineBrakesProportionalBrakeLag( 1 )
	EngineBrakesControllerMaxApplicationRate( 6 )
	EngineBrakesControllerMaxReleaseRate( 6 )
	EngineBrakesControllerEmergencyApplicationRate( 30 )
	EngineBrakesControllerMinSystemPressure( 0 )
	EngineBrakesControllerMaxSystemPressure( 90 )
	EngineBrakesControllerEmergencyBrakeTimePenalty( 0 )
	EngineBrakesControllerFullServicePressureDrop( 6 )

	TrainBrakesControllerMinPressureReduction( 2 )
	TrainBrakesControllerMaxApplicationRate( 2 )
	TrainBrakesControllerMaxReleaseRate( 2 )
        TrainBrakesControllerEmergencyApplicationRate( 30 )
	TrainBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMaxSystemPressure( 72.6 )
	TrainBrakesControllerEmergencyBrakeTimePenalty( 0 )
	TrainPipeLeakRate( 0.33 )
	
                
	BrakesEngineBrakeType ( "Air_single_pipe"  )
	BrakesTrainBrakeType ( "Air_single_pipe" )
	BrakesEngineControllers( "Independent, Train" )

        EngineBrakesControllerDirectControlExponent( 1 )

 MaxDieselLevel ( 1500l)
 DieselUsedPerHourAtMaxPower ( 102l)
 DieselUsedPerHourAtIdle ( 10l)
 DieselSmokeEffectInitialMagnitude ( 0.5)
 DieselSmokeEffectMaxMagnitude ( 1.5)
 DieselSmokeEffectInitialSmokeRate ( 0.5)
 DieselSmokeEffectMaxSmokeRate ( 5)
 DieselEngineIdleRPM ( 700)
 DieselEngineMaxRPM ( 1550 )
 DieselEngineMaxRPMChangeRate ( 100)
 DieselEngineSpeedOfMaxTractiveEffort ( 0.5mph)
 
 DoesHornTriggerBell ( 0)
 AWSMonitor (
  MonitoringDeviceMonitorTimeLimit ( -1)
  MonitoringDeviceAlarmTimeLimit ( 5)
  MonitoringDevicePenaltyTimeLimit ( 0)
  MonitoringDeviceCriticalLevel ( 0)
  MonitoringDeviceResetLevel ( 0)
  MonitoringDeviceAppliesFullBrake ( 0)
  MonitoringDeviceAppliesEmergencyBrake ( 1)
  MonitoringDeviceAppliesCutsPower ( 0)
  MonitoringDeviceAppliesShutsDownEngine ( 0)
 )
 EmergencyStopMonitor (
  MonitoringDeviceMonitorTimeLimit ( 0)
  MonitoringDeviceAlarmTimeLimit ( 0)
  MonitoringDevicePenaltyTimeLimit ( 0)
  MonitoringDeviceCriticalLevel ( 0)
  MonitoringDeviceResetLevel ( 0)
  MonitoringDeviceAppliesFullBrake ( 0)
  MonitoringDeviceAppliesEmergencyBrake ( 1)
  MonitoringDeviceAppliesCutsPower ( 0)
  MonitoringDeviceAppliesShutsDownEngine ( 0)
 )
 EngineControllers (
  AWS ( 0 1 0)
  BailOffButton ( 0 1 0)
  BellToggle ( 0 1 0)

 Brake_Engine ( 0 1 0.05 0
   NumNotches ( 1
    Notch ( 0 1 Dummy)
   )
  )
 comment(air brake "Knorr", driver's brake valve "ST60-11")
 Brake_Train ( 0 1 0.0125 0.4 
               NumNotches ( 5
                    Notch ( 0    0 TrainBrakesControllerReleaseStart )
                    Notch ( 0.1  0 TrainBrakesControllerRunningStart )
		    Notch ( 0.5  0 TrainBrakesControllerHoldLappedStart )
                    Notch ( 0.9  0 TrainBrakesControllerFullServiceStart )
                    Notch ( 1    0 TrainBrakesControllerEmergencyStart )
)
  )
  
 Throttle ( 0 1 0.125 0
 NumNotches ( 9
 Notch ( 0 0 Dummy )
 Notch ( 0.01 0 Dummy )
 Notch ( 0.03 0 Dummy )
 Notch ( 0.13 0 Dummy )
 Notch ( 0.25 0 Dummy )
 Notch ( 0.50 0 Dummy )
 Notch ( 0.67 0 Dummy )
 Notch ( 0.80 0 Dummy )
 Notch ( 1 0 Dummy )
 )
 ) 
  
  DirControl ( -1 0 1 1)
  EmergencyStopToggle ( 0 1 0)
  EmergencyStopResetToggle ( 0 1 0)
  Headlights ( 0 0.25 1 0)
  Horn ( 0 1 0)
  Sanding ( 0 1 0)
  Vigilance ( 0 1 0)
  Wipers ( 0 1 0)
 )
  Name ( "BKD Lxd2-255trfB" )
 Sound ( "Lxd2cab_wola.sms" )
 EngineVariables ( 333 )
 EngineOperatingProcedures ( 0 )
  Description ( "" )
)