SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( BKD_Zwora_Tw6a-Tw6a
 Type ( Freight )
 WagonShape ( BKDZworamiedzytransporterowa180cm.s )
  Name ( "BKD_Tw6a-zwora Tw6a-Tw6a-180cm[4c]" )
 Size ( 0.1m 0.3m 1.2m )
 Mass ( 1t )
 WheelRadius ( 29cm )
 InertiaTensor ( Box (0.1m 0.3m 1.2m) )
Coupling (
  Type ( Chain )
  Spring (
   Stiffness ( 7.5e6N/m 1e7N/m )
   Damping ( 1e6N/m/s 2e6N/m/s )
   Break ( 1.1e8N 5e8N )
   r0 ( 80cm 150cm )
          )
  CouplingHasRigidConnection ( 1 )
  Velocity ( 0.01m/s )
 )
 Buffers (
  Spring (
   Stiffness ( 7.5e6N/m 1e7N/m )
   Damping ( 1e6N/m/s 2e6N/m/s )
   r0 ( 20cm 30cm )
  )
  Centre ( 0.5 )
  Radius ( 1 )
  Angle ( 0.5deg )
 )
 Adheasion ( 0.2533   0.8233   2.5263   0 )
  comment ( Adhesion computed with NW 8 by TS-FastFix)
 DerailRailHeight ( 4cm )
 DerailRailForce ( 2.5*1t )
 DerailBufferForce ( 400kN )
 NumWheels(1)
 Friction (
  20N/m/s    -0.05    1.5mph    0.023N/m/s    1.999
  5.1N/rad/s    1        -1rad/s   0             1
  )

 BrakeEquipmentType ( "Triple_valve" )
 BrakeSystemType ( "Air_single_pipe" )
 MaxBrakeForce( 0kN )

 TripleValveRatio( 0 )
 MaxReleaseRate( 2.5 )
 MaxApplicationRate( 2.5 )
 BrakeCylinderPressureForMaxBrakeBrakeForce( 50.76 )
)